**talento smart CE2 (channel extension)**

**Digital extension module for S25, 2-channel extension, integrated Bluetooth,**

**programming by app, 2TE**

Extension module with integrated Bluetooth interface for talento smart S25 digital distributor time switch. No additional hardware required for program transfer. Protection against tampering provided by encrypted data transmission, PIN protection and product’s ability to be sealed. Daily, weekly and annual programs with 800 freely combinable switch commands. Shortest switching time 1 second. ON/OFF, pulse, cycle, sunrise/sunset-dependent switch commands, random switch commands.

Supply voltage 110–230 V, 50–60 Hz; switching capacity: 2 potential-free changeover contacts with zero crossing detection 16 A/250 V AC; 600 W LED load; captive screw terminal with wire protection max. 2.5 mm²; high-resolution dot-matrix display with background lighting; automatic operation, fix ON/OFF, override; Dimensions 90 x 35.5 x 60 mm (H x W x D)

Manufacturer: Grässlin

Model: talento smart CE2

Item no.: 43.04.0004.1